#

## § 45.2-730 – Signs, life lines, and equipment

##

A. Direction signs shall be posted conspicuously at all points where a travel way to the mine opening, escapeway, or escapement shaft is intercepted by another travel way. The signs shall indicate the direction of the place of exit and any manway or escapeway.

B. Continuous life lines shall be installed and maintained in accordance with the approved emergency response plan pursuant to subsection A of § 45.2-820.

C. Every escapeway shall be equipped with all necessary stairways, ladders, cleated walkways, or other equipment approved by the Chief. All equipment shall be installed in such a manner that a person using it in an emergency may do so quickly and without undue hazard.